# Amplifiers

### Explanation of question 8

When a transmitter is operating in class B, output current flows

1. all the time
2. two-thirds of the time
3. one-half of the time
4. one-quarter of the time

The answer is :- 3 One-half of the time, hence the use of push-pull or a complementary pair.

BACK

page (tq1508ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details