# Section 8 - Operating Practices & Procedures

## 20m (14MHz) Band plan

14MHz (20m) | Licence | Amateur Service: Primary
Notes: | Amateur Satellite Service: 14000 - 14.250 Primary
|  |  | Permitted Modes: Morse, telephony, RTTY, data, fax, SSTV
IARU | UK Usage
14.000 |  |  |  | 14.000 - 14.060 14.060 | CW only contest preferred segment
CW only
14.070 | 14.089 - 14.099 | No digimode mailbox or forwarding AX25 packet preferred frequencies
Digimodes (and CW)
14.099 | 14.099 - 14.101 | Reserved exclusively for beacons
Beacons Only
14.101 | 14.101 - 14.112 | Digimode mailbox and forwarding AX25 packet preferred frequencies
Digimodes (+ phone and CW)
14.112 | 14.125 - 14.300 14.230 14.285 | SSB only contest preferred segment SSTV/fax calling frequency QRP
Phone (and CW)
14.350

Back | Index | Next