The Amateur Radio Project - Measurements

# Measurements

### Question 28 of 32

A method of measuring the output power of an SSB transmitter with an oscilloscope requires the use of

1. an RF oscillator
2. a two-tone RF oscillator
3. an AF oscillator
4. a two-tone AF oscillator

1 | 2 | 3 | 4

Back |

page (tq2328)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details