The Amateur Radio Project - Diodes and their applications

# Diodes and their applications

### Question 5 of 14

In the circuit in Fig. 13.1, the ammeter indicates a current starting to flow when the voltmeter reads 0.6V. The junction diode will be

1. germanium, forward-biased
2. germanium, reverse-biased
3. silicon, forward-biased
4. silicon, reverse-biased

1 | 2 | 3 | 4

Back |

page (tq1305)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details