# Section 5 - Antennas & Feeders

In order to transmit or receive a signal, we must connect our radio transmitter or receiver to an antenna (Note that in this text and in the assessment we shall use the word "antenna" rather than "aerial"). The antenna is connected top the radio by a cable known as a feeder.

In order for us to be able to choose a suitable antenna and set it up correctly it is important that we learn a little about them.

## 5.1 - 5.2 Feeders

The feeder is the cable that connect the radio to the antenna. When transmitting it must carry a powerful radio signal from the transmitter to the antenna without radiating any of that signal itself. When receiving, it must carry the very weak signal from the antenna to the receiver without allowing any other (interfering) signals to be picked up by the feeder. For this reason, the most common feeder you will come across is coaxial cable.

Coaxial cable consists of a core which may be solid or multi-stranded surrounded by an insulating material known as the dielectric. Around this is a screen usually consisting of many very thin wires braided to form a tight covering over the dielectric. The purpose of this screen is to keep the signal within the cable, so it must be continuous and will usually completely cover the dielectric. The screen is protected from the elements by an outer jacket of flexible plastic, normally PVC.

In order that we can maintain the screen all the way from radio to antenna, we will use a connector that has a similar structure to the coaxial cable. It will have a centre conductor, the pin, surrounded by an insulator and the connector body will be metal to provide the screen. The two most common types of coaxial connectors used are the PL259 and BNC connectors. The coaxial cable screen must be securely connected to the metal body of the connector in order that we can maintain the desired continuous screen from radio to antenna. The centre conductor of the coaxial cable is crimped or soldered to the centre pin of the connector.

Note that the PL259 is significantly larger than the BNC.

Back | Index | Next