The Amateur Radio Project - Measurements

# Measurements

### Question 8 of 32

A moving coil milliammeter has a resistance of 9 and an f.s.d. of 1mA. When used with a shunt of resistance 1 the instrument will read up to

1. 11mA
2. 10mA
3. 9mA
4. 1.11mA

1 | 2 | 3 | 4

Back |

page (tq2308)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details