The Amateur Radio Project - F.M., A.M. and S.S.B. transmitters

# F.M., A.M. and S.S.B. transmitters

### Question 12 of 24

A modulation factor (modulation depth) greater than unity in an AM transmitter is

1. desirable- it indicates maximum output power is achieved
2. desirable- it indicates sufficient audio from the microphone
3. undesirable- it indicates a too large deviation of the carrier frequency
4. undesirable- it indicates possible distortion

1 | 2 | 3 | 4

Back |

page (tq1812)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details