The Amateur Radio Project - Licencing conditions

# Licensing conditions

### Question 16 of 40

The transmitter in an amateur radio station is only used for transmitting single sideband signals in the 20m and 10m bands. The station must have a receiver capable of receiving

1. SSB and AM signals in the 20m and 10m bands
2. SSB signals in the 20m and 10m bands
3. SSB signals in all the HF bands (160m to 10m)
4. SSB signals in all the HF bands and 2m FM signals

1 | 2 | 3 | 4

Back |

page (tq2616)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details