The Amateur Radio Project - Transformers

# Transformers

### Question 1 of 8

A 240V to 24V step-down transformer takes a no-load primary current of 0.1A. The secondary current on no load will be

1. 1A
2. 0.1A
3. 0.01A
4. zero

1 | 2 | 3 | 4

Back |

page (tq1101)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details