The Amateur Radio Project - F.M., A.M. and S.S.B. transmitters

# F.M., A.M. and S.S.B. transmitters

### Question 19 of 24

Both sidebands from the balanced modulator of an SSB transmitter are fed through a filter. The typical bandwidth of the filter will be

1. 2.5kHz
2. 5kHz
3. 2.5MHz
4. 5MHz

1 | 2 | 3 | 4

Back |

page (tq1819)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details