# Amplifiers

### Explanation of question 6

The practical operating efficiency of a class A amplifying stage is

1. less than 30%
2. 50—70%
3. 70—85%
4. 85—100%

The answer is :- 1 Class A has low efficiency. Less than 25% is typical.

BACK

page (tq1506ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details