The Amateur Radio Project - Practical resistors

# Practical resistors

### Question 5 of 6

A 47 resistor takes a current of 100mA. Its preferred power rating should be of a value at least

1. 1/2W
2. 1/4W
3. 1/8W
4. 1/10W

1 | 2 | 3 | 4

Back |

page (tq0405)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details