The Amateur Radio Project - Capacitance

# Capacitance

### Question 6 of 10

The circuit between A and B in Fig. 6.1 can be replaced by a single resistor in series with a single capacitor. Their values will be, respectively,

1. 12, 4.8 mfd
2. 12, 20 mfd
3. 32, 4.8 mfd
4. 32, 20 mfd

1 | 2 | 3 | 4

Back |

page (tq0606)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details