The Amateur Radio Project - F.M., A.M. and S.S.B. transmitters

# F.M., A.M. and S.S.B. transmitters

### Question 22 of 24

The output from the filter of a sideband generator is at 9MHz. It is mixed with that of a VFO covering 5- 5.5MHz. Two amateur bands that can be covered are

1. 20m and 80m
2. 20m and 15m
3. 15m and 80m
4. 10m and 20m

1 | 2 | 3 | 4

Back |

page (tq1822)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details