The Amateur Radio Project - Receivers

# Receivers

### Question 20 of 22

The carrier insertion oscillator in an SSB receiver is to

1. facilitate receiver calibration
2. provide a signal to a mixer to generate the intermediate frequency
3. remove the carrier to give single sideband reception
4. insert a carrier for the reception of single sideband transmission

1 | 2 | 3 | 4

Back |

page (tq2220)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details