# Oscillators

### Explanation of question 3

In Fig. 16.1, to change the oscillator frequency, adjustment is normally made to

1. C1 and C2
2. C4 and C5
3. R
4. L

The answer is :- 1

3 Adjustment to frequency is made by C1 (variable) and C2 (preset).

BACK

page (tq1603ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details