The Amateur Radio Project - Operating procedures and practices

# Operating procedures and practices

### Question 18 of 21

For safety reasons a bleeder resistor is connected across a 0.5 1F capacitor. It should have a value

1. less than 500k
2. between 500k and 5M
3. between 5M and 10M
4. greater than 10M

1 | 2 | 3 | 4

Back |

page (tq2518)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details