# Amplifiers

### Explanation of question 15

The output frequency of a doubler is to be 144MHz. The input frequency must therefore be

1. 288MHz
2. 72MHz
3. 48MHz
4. 36MHz

The answer is :- 2 Output = 144 MHz, therefore input = 144/2 MHz = 72 MHz.

BACK

page (tq1515ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details