The Amateur Radio Project - C.W. transmitters and keying

# C.W. transmitters and keying

### Question 6 of 10

Fig. 17.3 represents the output circuit of a power amplifier for a VHF. transmitter. The circuit

- i will act as a high-pass filter
- ii will act as a low-pass filter
- iii can be used for matching

1. i and iii are true
2. ii and iii are true
3. i is true but iii is false
4. ii is true but iii is false

1 | 2 | 3 | 4

Back |

page (tq1706)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details