The Amateur Radio Project - Amplifiers

# Amplifiers

### Question 8 of 18

When a transmitter is operating in class B, output current flows

1. all the time
2. two-thirds of the time
3. one-half of the time
4. one-quarter of the time

1 | 2 | 3 | 4

Back |

page (tq1508)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details