The Amateur Radio Project - Transmitter interference

# Transmitter interference

### Question 16 of 17

An HF transmitter is capable of transmitting in all the allocated bands from 80m to 10m. A suitable filter to connect between the transmitter and antenna would be a

1. 30MHz cut-off high-pass filter
2. 30MHz cut-off low-pass filter
3. 3MHz cut-off high-pass filter
4. 3MHz cut-off low-pass filter

1 | 2 | 3 | 4

Back |

page (tq2416)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details