The Amateur Radio Project - Measurements

# Measurements

### Question 31 of 32

A digital frequency meter of accuracy 4 parts per 100,000 is used to check the frequency of operation of a transmitter in the 10m band. The most accurate reading will be

1. 28.09MHz
2. 28.094MHz
3. 28.0946MHz
4. 28.1MHz

1 | 2 | 3 | 4

Back |

page (tq2331)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details