# Safety precautions in the amateur station

## RSGB Mobile Safety Recommendations

1. All equipment should be so constructed and installed that in the event of accident or sudden braking it cannot injure the occupants of the vehicle.
2. Mobile antennas should be soundly constructed, taking into account flexing at speed and possible danger to other vehicles or pedestrians. The maximum height must not exceed 14ft above ground.
3. Wiring should not constitute a hazard, either electrical or mechanical, to driver or passengers.
4. All equipment should be adequately fused and a battery isolation switch is desirable.
5. The transmit/receive switch should be within easy access of the operator and one changeover switch should perform all functions.
6. The microphone should be attached to the vehicle so that it does not impair the vision or movement of the driver.
7. The driver/operator should not use a hand microphone or double headphone.
8. All major adjustments, for example a band change by a driver/operator, should be carried out while the vehicle is stationary.
9. Essential equipment controls should be adequately illuminated during the hours of darkness.
10. All equipment must be switched off when (a) fuelling, (b) in close proximity to petrol tanks and (c) near quarries where charges are detonated electrically.
11. A suitable fire extinguisher should be carried and be readily accessible.

Back | Index | Next