The Amateur Radio Project - Measurements

# Measurements

### Question 7 of 32

A moving coil microammeter has an f.s.d. of 200A and resistance 20. The value of shunt resistance required such that the instrument will have an f.s.d. of 1mA is

1. 5
2. 4
3. 3.33
4. 0.20

1 | 2 | 3 | 4

Back |

page (tq2307)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details