The Amateur Radio Project - Diodes and their applications

# Diodes and their applications

### Question 9 of 14

A full-wave bridge rectifier is correctly connected to a 6V, 50Hz supply. The ripple frequency will be

1. 200Hz
2. 100Hz
3. 50Hz
4. 25Hz

1 | 2 | 3 | 4

Back |

page (tq1309)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details