# C.W. transmitters and keying

### Explanation of question 3

The driver and power amplifier of a c.w. transmitter will normally be operating in class

1. A
2. AB
3. B
4. C

The answer is :- 4 For c.w. operation, the high efficiency class C will normally be adopted.

BACK

page (tq1703ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details