    AST RESEARCH, INC.         TECHNICAL BULLETIN #0851               08-04-93

                   BRAVO LC 4/66 WITH LOTUS 123 v2.4 WILL NOT BEEP

    PROBLEM:       Lotus 123 version 2.4 will not beep if loaded on a Bravo LC
                   4/66.

    CAUSE:         The fault lies within the Lotus program.  The software signals
                   sent out are not quick enough for the system to interpret
                   them.

    AFFECTED
    SYSTEMS:       Bravo LC 4/66.

    SOLUTION:      None. Lotus is aware of the problem but is not going to fix
                   this particular version.  Slowing the machine down when
                   running the program was their only suggestion.