    AST RESEARCH, INC.         TECHNICAL BULLETIN #0862               08-19-93

                   POWER EXEC DRIVE BAY ADAPTER AND 8-BIT DEVICES

    The Power Exec Drive Bay Adapter can be configured to function as an 8-bit or
    16-bit device.  By default, the Drive Bay Adapter is set for 16-bit
    operation, however, when installed in a system that has 8-bit video, the
    Drive Bay Adapter must be set for 8-bit operation.

    By definition, the IBM PC/AT Specification dictates that an 8-bit device
    cannot co-exist with a 16-bit device in the same memory region.  Therefore,
    if the system's video is an 8-bit device, then the Drive Bay Adapter will
    work only if set to 8-bit operational mode.