    =

    AST RESEARCH, INC.       TECHNICAL BULLETIN # 1288                 11-22-95

    =

            Bravo MS Fails to Boot with Videologic 928Movie Video Adapter

    PROBLEM

    Bravo MS with Videologic 928Movie video adapter may not perform a cold boot.

    CAUSE

    The system board signals on the ISA bus combined with the reset conditioning
    circuit of the 928Movie, cause the video adapter to not be initialized.

    SOLUTION

    Contact Videologic's Technical Support at (415) 875-0606 with reference to
    Field Note 181 or CompuServe: Go Videologic.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501442-006      Bravo MS 4/66D