    AST RESEARCH, INC.         TECHNICAL BULLETIN #0747                  02-21-92

                        RAMPAGEPLUS/MC AND DCA 3270/MC BOARD

    PROBLEM:       When installing a DCA 3270/MC board in an IBM PS/2 system with
                   a RampagePlus/MC board already installed, after completing the
                   DCA 3270 installation, the memory previously supplied by the
                   RampagePlus/MC board will no longer be counted during post.

    CAUSE:         The ASTART.EXE program supplied with the RampagePlus/MC board
                   does not correctly register memory on the IBM reference disk,
                   which allows the DCA 3270/MC board to corrupt the
                   RampagePlus/MC memory configuration.

    SOLUTION:      Use the ASTART.EXE (version 1.21.01) available on the AST On-
                   Line! BBS.  (This is not an AST released driver, and AST makes
                   no warranty regarding the usability of this driver).