    =

    AST RESEARCH, INC.            TECHNICAL BULLETIN # 1037               12-15-94

    =

         INSTALLING A THIRD HARD DISK DRIVE IN PREMMIA LX AND ADVANTAGE! EXP60

            This is an informational bulletin.

            The procedure below states how to install a third hard disk drive in
            the Premmia LX and Advantage! EXP systems with system board part
            number 230822-002.

            1. Update to BIOS release. 1.11.  File 537034.EXE can be found on
               AST's BBS in the Systems file area.  AST's BBS can be reached by
               dialing the following telephone number: (817) 230-6850.  AST's
    	   BBS supports modem speeds up to 28.8k bps.

            2. Run CMOS Setup.
            3. Select "Advanced".
            4. Select "Peripheral Configuration".
            5. Set Configuration Mode to "Manual".
            6. Enable both PCI and Standard IDE Interface options.
            7. Exit and Save.

            The Premmia LX and Advantage! EXP systems will detect the third drive
            and display it as E: during POST.  The drive can then be accessed
            through DOS as drive E:.

            NOTE:  Step five must be followed even though the port may show as
            being enabled when mode is set to Auto.

            NOTE: The data transfer rate is considerably slower through the
            Standard port.

            NOTE:  The system must have the -002 system board.  The -001 system
            board does not contain the RZ1000 PCI to IDE I/O chip, even though the
            PCI IDE connector may be in place on some -001 system board revisions.

    SYSTEMS
    AFFECTED:   AST
            PART NUMBER      DESCRIPTION

            501288-XXX      PREMMIA LX P/60
            501289-XXX      PREMMIA LX P/66
            501422-XXX      ADVANTAGE EXP60