    AST RESEARCH, INC.         TECHNICAL BULLETIN #0880                 12-8-93

                        BRAVO LC2 KEYBOARD LED'S DO NOT FLASH

    PROBLEM:       When the "SERVER" password mode is enable in CMOS setup, the
                   keyboard LED's don't flash as stated in the User's Manual
                   (part number 001796-001).  The manual states that the Num
                   Lock, Caps Lock, and Scroll Lock lights flash upon booting the
                   system, before the password is entered.

    CAUSE:         The keyboard controller used in this system cannot be
                   programmed to control the keyboard LED's.

    AFFECTED
    SYSTEMS:       All models of Bravo LC2 systems.

    SOLUTION:      This situation is a function of system design and there is no
                   method of making the LED's flash with a password set.