    AST RESEARCH, INC.         TECHNICAL BULLETIN #0826               04-22-93

                          PENEXEC AND PCMCIA CONFIGURATION

    For some users who wish to add a PCMCIA Modem card, it is important to
    configure system Setup correctly (select CONFIGURE SYSTEM from Executive Menu
    after exiting Windows, or, PADMENU from the UTILS directory on the hard
    drive).  In some early systems, a field in Setup called Enable Modem is
    displayed.  This field MUST be set to DISABLE for the PCMCIA Modem to operate
    correctly.

    The PCMCIA software driver diskette that was included with the PCMCIA Modem
    must be version 1.04 or above (AST part number 910717-033).  If necessary,
    contact AST Product Support for information on obtaining the correct version.

    After installing the PCMCIA driver software, make sure that the output port
    is configured as COM2.  Check your CONFIG.SYS file for the following
    statement:

         DEVICE=C:\ASTCCU\CCU.EXE/COMM=2