    =

    AST RESEARCH, INC.          TECHNICAL BULLETIN # 1346               12-8-95

    =

    		      Correction To Premmia LX User Manual

    This is an informational bulletin.

    Pages 5 through 7 of the AST Premmia LX User's Manual
    (P/N 001979-001A, October 1993) state the following:

         "The system contains tin-plated SIMM sockets.  Only install SIMMs with
           tin-plated leads in the system".

    The above is an incorrect statement.  Both tin-plated and gold-plated SIMMs
    can be used in the Premmia LX.  Mixing combinations of the two types is
    acceptable as long as they are installed in pairs.

    Future revisions of this manual will correct the error.  For the approved
    SIMM Vendor List, see Technical Bulletin # 0899.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501288          Premmia LX Pentium/60    All Models
    501289          Premmia LX Pentium/66    ALL