    =

    AST RESEARCH, INC.        TECHNICAL BULLETIN # 1102                 3-15-95

    =

    			  INCORRECT BRAVO MS SPEED JUMPER SETTINGS

    PROBLEM

    The Bravo MS Hardware Maintenance Manual (P/N 002092-001, section 3-2) and the
    User's Manuals (P/N 002115-001, page 59) incorrectly state the E9 jumper
    settings as:

    	ON= 33MHz
    	OFF= 25MHz

    CAUSE

    Print error.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501442-XXX     BRAVO MS 4-66D
    501443-XXX     BRAVO MS 4-100T
    501586-XXX     BRAVO MS-L 4-66D
    501658-XXX     BRAVO MS-T 4-66D

    SOLUTION

    The following are the correct jumper settings:

    E9 Jumper:
    	ON= 25MHZ
    	OFF= 33MHz

    E6   E7 Jumper
    1/2  1/2  25MHz
    1/2  2/3  33MHz
    All other combinations are reserved.