    =

    AST RESEARCH, INC.          TECHNICAL BULLETIN # 1396                1-8-96

    =

        Installing Windows NT 3.51 with Quad Speed CD-ROM on Manhattan Server

    PROBLEM

    When installing Windows NT 3.51 from CD-ROM, with the Sanyo CRD254S CD-ROM,
    on the integrated NCR SCSI controller, bad or corrupt files may occur during
    the file copy process.

    CAUSE

    The NCR driver version that ships with Windows NT 3.51 does not work properly
    with the CD-ROM.

    SOLUTION

    Download the latest driver (version 2.00.00) from SymBios Logic's BBS at
    (719) 573-3562, file name NT35_DRV.ZIP, or you may obtain the driver from
    SymBios Logic's ftp sight at:

    	 ftp.symbios.com/pub/ncrchips/scsi/drivers/Win_NT35/nt35_drv.zip

    SYSTEMS AFFECTED
    AST PART NUMBER and DESCRIPTION

    501500-XXX      Manhattan V5090
    501502-XXX      Manhattan P5090
    501503-XXX      Manhattan P5100
    501830-XXX      Manhattan P5133