    AST RESEARCH, INC.         TECHNICAL BULLETIN #1304              9-13-95

            386 MAX VERSION 7.00 / 7.01 WITH ADVANTAGE / BRAVO PENTIUM

    PROBLEM:     When loading the 386MAX driver the system will continually
                 reboot.

    CAUSE:       The failure is caused when the driver loads the "machine
                 check exception" routine in CR4.

    SOLUTION:    Update the present version of 386 Max to version 7.02.  For
                 users who have version 7.00 installed, download and install
                 the file M700702.EXE.  For users who have version 7.01
                 installed, download and install the file M701702.EXE

                 The Qualitas BBS can be reached by dialing (301) 907-8030.