    AST RESEARCH, INC.	TECHNICAL BULLETIN #1274	8-17-95

    AST PCMCIA ETHERNET CARD ON ASCENTIA 950N

    This is an informational bulletin.

    Unable to connect an Ascentia 950N system to a network with an add-in AST
    PCMCIA Ethernet card.

    The Ascentia 950N User’s Manual on page 67 states:

    Card and Socket Services assigns the following default parameters to a
    PCMCIA network card:

    	IRQ 	I/O Address	Memory Address
    	5	300h-31Fh	D400h-D7FFh

    If you are installing an AST Ethernet card, change the IRQ settings to 9.
    When installing the network drivers, you must match the settings of Card
    and Socket Services.

    SYSTEMS AFFECTED:

    AST Part Number	Description

    501707-2XX	Ascentia 950N/75N CSS10 510/8
    501707-3XX	Ascentia 950N/75N CSS10 700/8
    501707-4XX	Ascentia 950N/75N CSS10 1G/8
    501708-3XX	Ascentia 950N/75N CTS10 700/8
    501708-4XX	Ascentia 950N/75N CTS10 1G/8