    =

    AST RESEARCH, INC.        TECHNICAL BULLETIN # 1355                 11-9-95

    =

              Ascentia 950N Will Not Fill Screen on Overhead Projector

    PROBLEM

    When running Windows 95 on an Ascentia 950N which is connected to a
    Proxima LCD overhead projector, the display will only fill half of the screen
    at a time.  The Ascentia 950N BIOS used is version 2.57.

    CAUSE

    This version of the Ascentia 950N BIOS does not support expanded font
    mode.

    SOLUTION

    Update the Ascentia 950N BIOS to version 2.58 (p/n 905557-039).

    File 05557039.EXE can be found on AST's BBS (817) 230-6850.
    AST's BBS supports modem speeds up to 28.8k bps.  The above file will also
    be posted on:

    CompuServe
    Go ASTSUPPORT

    AST Worldwide Web Site
    http://www.ast.com

    For additional information on the Ascentia 950N system BIOS, see Software
    Bulletin 0246 on AST's BBS and other On-Line forums.

    SYSTEMS AFFECTED
    AST PART NUMBER AND DESCRIPTION

    501707-XXX      Ascentia 950N P/75 CSS10
    501708-XXX      Ascentia 950N P/75 CTS10