    =

    AST RESEARCH, INC.          TECHNICAL BULLETIN # 0968A              9-27-94

    =

                        PREMMIA MX AND PREMMIA GX COM4 CONFLICT

    PROBLEM:         The system hangs when a COM port or other device is configured
                     to use I/O address 2E8-2EF (8 bytes) on the Premmia MX or
                     Premmia GX system.

    CAUSE:           The ATI Mach 64 card uses I/O port 2EC, creating a conflict.

    SYSTEMS
    AFFECTED:            AST                                              REVISION
                     PART NUMBER        DESCRIPTION                         LEVEL

                     501457-XXX      PREMMIA GX P/90                         All
                     501522-XXX      PREMMIA GX P/100                        All
                     501429-XXX      PREMMIA MX 4/66d                        All
                     501432-XXX      PREMMIA MX 4/100t                       All
                     501577-XXX      PREMMIA MX P/60                         All

    SOLUTION:       Do not use COM4 or other devices which use I/O port 2E8h when
                    the Mach64 video card is installed in the system.  If it
                    becomes necessary to install a device which must use I/O port
                    2E8h, there are other video cards that do not conflict with
                    this port.