    =

    AST RESEARCH, INC.         TECHNICAL BULLETIN # 1068                 2-9-95

    =

    				 PREMMIA GX, MX FLOPPY DISK DRIVE CABLE

    PROBLEM
    When installing certain floppy devices on Premmia GX and Premmia MX systems,
    the AST-supplied cable may not have sufficient length to secure a proper
    connection.

    SOLUTION
    If installing a floppy drive with a drive cable on the right side, use
    P/N 220085-009 CABLE ASSY FLOPPY 3.5/5.25 (25L).