    =

    AST RESEARCH, INC.        TECHNICAL BULLLETIN # 1057                1-25-95

    =

    				   BRAVO LC 4-66D OS/2 AND NETX.EXE

    PROBLEM
    When entering a DOS private session under OS/2 2.1 and executing NETX to
    access the file server, the Bravo LC system hangs.

    CAUSE
    The OS/2 2.1 CSD (Corrective Service Diskette) level is at 1020.

    SYSTEMS AFFECTED
    AST PART NUMBER    DESCRIPTION

    501380-005        BRAVO LC 4-66D

    SOLUTION
    Install the OS/2 Service Pack which brings the CSD level to 6200.  To do this,
    follow the steps below:

    1. Access CompuServe.
    2. Type "Go OS2SERVICE".
    3. Select the Service Pack (3.5" or 5.25") required and download all the
       diskettes in that section.
    4. Install the diskettes over the current OS/2 installation.
    5. Reboot the system.