    AST RESEARCH, INC.            TECHNICAL BULLETIN #0901                3-8-94

                              PREMMIA LX ADAPTER ERRORS

    PROBLEM:       When UB diagnostics are run you will receive error 02 if the
                   shadow is disabled.  You will receive error FF if the shadow
                   is enabled for the range of the adapter.

    CAUSE:         The system (adapter) is not configured properly or is not
                   installed.  Possible HW problem on card.

    SYSTEMS
    AFFECTED:      PREMMIA LX.

    SOLUTION:      Enter the advanced CMOS setup and disable the cache.