DOS/32 Advanced DOS Extender - Programmer's Reference 2.10 - DPMI function 000Bh - Get Descriptor Copies the descriptor table entry for the specified selector into an 8-byte buffer.
In: | AX = 000Bh BX = selector ES:EDI = selector:offset of 8-byte buffer
Out: | if successful: CF clear the buffer pointed to by ES:EDI contains descriptor if failed CF set AX = error code 8022h - invalid selector
Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.