DOS/32 Advanced DOS Extender - Programmer's Reference 3.24 - DOS function 4Ah - Resize DOS Memory
In: | AH = 4Ah EBX = new memory block size in paragraphs ES = selector of previously allocated memory block
Out: | if successful: CF clear if failed: CF set EAX = DOS error code EBX = maximum paragraphs available for specific memory block
Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.