DOS/32 Advanced DOS Extender - Programmer's Reference 3.53 - DOS function 0FF95h - DOS/32 Advanced Allocate Low Memory Block
In: | AX = 0FF95h EBX = size of memory block in bytes
Out: | if successful: CF clear EBX = linear address of allocated memory block ESI = handle of allocated memory block if failed: CF set
Notes: a) This call is specific to DOS/32 Advanced DOS Extender only, and is not supported by standard DOS. b) This function works in exactly the same way as extended DOS function 0FF91h except that it allocates a DOS memory block. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.