DOS/32 Advanced DOS Extender - Programmer's Reference 2.12 - DPMI function 000Eh - Get Multiple Descriptors Copies one or more descriptor table entries into a client buffer.
In: | AX = 000Eh CX = number of descriptors to copy ES:EDI= selector:offset of a buffer in the following format:
Offset | Length | Contents
00h | 2 | Selector #1 (set by client)
02h | 8 | Descriptor #1 (returned by host)
0Ah | 2 | Selector #2 (set by client)
0Ch | 8 | Descriptor #2 (returned by host)
. . . | . . . | . . .
Out: | if successful: CF clear the buffer contains copies of the descriptors for the specified selectors if failed: CF set AX = error code CX = number of descriptors successfully copied 8022h - invalid selector
Notes: a) If an error occurs because of an invalid selector or descriptor, the function returns the number of descriptors which were successfully copied in CX. All of the descriptors which were copied prior to the one that failed are valid. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.