DOS/32 Advanced DOS Extender - Programmer's Reference 2.02 - DPMI function 0001h - Free Descriptor Frees a descriptor.
In: | AX = 0001h BX = selector for the descriptor to free
Out: | if successful: CF clear if failed: CF set AX = error code 8022h - invalid selector
Notes: a) Each descriptor allocated with DPMI function 0000h must be freed individually with this function, even if it was previously allocated as part of a contiguous array of descriptors. b) DOS/32 Advanced DPMI and DPMI 1.0 hosts will zero any segment registers which contain the selector specified in register BX. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.