DOS/32 Advanced DOS Extender - Programmer's Reference 5.08 - Mouse function 0020h - Enable Mouse Driver
In: | AX = 0020h
Out: | AX = 0020h on error AX = 0FFFFh on success
Notes: a) This function will always return AX=0FFFFh to be compatible with DOS/4GW DOS Extender. b) The protected mode program should not rely on error codes reported by this function in AX register since different mouse drivers will return different values on error. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.