README.VRS                  11/29/89
The following GRAPHIC DRIVERS are included on this diskette. 
These .VRS files are broken down into three categories (Shipping
With WordPerfect 5.1, Extracted From STANDARD.VRS, and Additional
Graphic Drivers).  Each .VRS file is listed along with a brief
description of the video card(s) the file is designed to drive. 
Certain .VRS files also include text drivers which are listed in
parentheses on the following line.

Category 1:  Shipping With WordPerfect 5.1

With the exception of STANDARD.VRS, these are the graphics/text
screen drivers currently shipping with WordPerfect 5.1.

.VRS FILE      VIDEO CARD                        RESOLUTION/COLOR
-----------------------------------------------------------------
8514A.VRS      IBM 8514 Adapter               1024x768, 265 color

ATI.VRS        ATI VIP VGA                      800x560, 16 color
               ATI EGA Wonder                       (text driver)
               (132x25, 16 color; 132x25, mono;
               132x44, 16 color; 132x44, mono)

GENIUS.VRS     MDA Genius 1               736x1008, Mono Portrait
               (default)
               MDA Genius 2                  1280x1024, Mono Dual
               (default; 128x66; 128x72; 
               128x85; 140x66; 140x72;
               140x85; Dual 80x66)

INCOLOR.VRS    Hercules InColor                 720x348, 16 color

PARADISE.VRS   Paradise AutoSwitch EGA          640x480, 16 color
               Paradise VGA Plus               640x400, 256 color
                                                640x480, 16 color
                                                800x600, 16 color
               (132x25, 16 color; 132x25, mono;
               132x44, 16 color; 132x44, mono)

VIDEO7.VRS     Video 7 VGA                      800x600, 16 color


Category 2:  Extracted from STANDARD.VRS

STANDARD.VRS contains several of the most common graphic/text
screen drivers combined into one file.  These files are the
individual drivers extracted from STANDARD.VRS.  These files are
provided for users with two floppy drive systems who require
additional disk space for program operation.  These drivers and
STANDARD.VRS are designed to be used separately.  Therefore,
STANDARD.VRS should be removed before copying any of these
drivers to your working program diskette.

.VRS FILE      VIDEO CARD                        RESOLUTION/COLOR
-----------------------------------------------------------------
S_MCGA.VRS     IBM MCGA                        320x200, 256 color
               IBM VGA                         320x200, 256 color

S_CGA.VRS      AT&T                                 640x400, Mono
               Compaq Portable Plasma               640x400, Mono
               IBM CGA                           640x200, 2 color
               IBM VGA                           640x480, 2 color
               Toshiba T3100
               Toshiba T5100

S_EGA.VRS      IBM EGA                          640x200, 16 color
                                                640x350, 16 color
                                                 640x350, 2 color
                                           640x350, 4 color (64K)
                                                640x480, 16 color

S_VGA.VRS      IBM VGA                          640x480, 16 color

S_HERC.VRS     Hercules                             720x348, Mono

S_TIBM.VRS     IBM EGA                              (text driver)
               (80x25, 16 color;
               80x43, 16 color;
               80x43, 16 color, cursor;
               80x43, 16 color Save Font;
               80x43, 16 color Save Font, cursor)
               IBM VGA                              (text driver)
               (80x25, 16 color;
               80x28, 16 color Save Font;
               80x43, 16 color Save Font;
               80x50, 16 color;
               80x50, 16 color; Save Font)

S_THERC.VRS    Hercules Ramfont                     (text driver)
               (80x25 Mono;
               80x25 Mono Save 4k Font;
               80x25 Mono Save 4k Font in WP;
               80x43 Mono
               80x43 Mono Save 4k Font)

Category 3:  Additional Graphic Drivers

These are the additional graphics/text screen drivers currently
available which do not ship with the standard WordPerfect 5.1
software package.

.VRS FILE      VIDEO CARD                        RESOLUTION/COLOR
-----------------------------------------------------------------
GENOA.VRS      Genoa VGA                       640x480, 256 color
                                     800x600, 16 color (MODE 29H)
               Genoa SuperVGA                       (text driver)
               (132x25, 16 color Save Font;
               132x29, 16 color Save Font;
               132x32, 16 color Save Font; 
               132x44, 16 color Save Font;
               132x60, 16 color Save Font;
               Default)

GTEXT.VRS      Text (No Graphics)

NEC.VRS        NEC GB-1                         640x480, 16 color

WYSE.VRS       WYSE Wy-700                         1280x800, Mono